###############################################################################
#
# IAR ELF Linker V8.30.1.114/W32 for ARM                  29/Aug/2021  17:01:11
# Copyright 2007-2018 IAR Systems AB.
#
#    Output file  =  
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Exe\MT_ENC28J60.out
#    Map file     =  
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\List\MT_ENC28J60.map
#    Command line =  
#        -f C:\Users\Aveal\AppData\Local\Temp\EW9BFE.tmp
#        (D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\enc28j60.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\main.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\startup_stm32f103xb.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_cortex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_dma.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_exti.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_flash.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_flash_ex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_gpio.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_gpio_ex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_msp.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_pwr.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_rcc.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_rcc_ex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_spi.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_tim.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_hal_tim_ex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\stm32f1xx_it.o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj\system_stm32f1xx.o
#        --redirect _Printf=_PrintfFull --redirect _Scanf=_ScanfFull
#        --no_out_extension -o
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Exe\MT_ENC28J60.out
#        --map
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\List\MT_ENC28J60.map
#        --config
#        D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM/stm32f103xb_flash.icf
#        --semihosting --entry __iar_program_start --vfe --text_out locale)
#
###############################################################################

*******************************************************************************
*** RUNTIME MODEL ATTRIBUTES
***

CppFlavor       = *
__SystemLibrary = DLib
__dlib_version  = 6


*******************************************************************************
*** HEAP SELECTION
***

The basic heap was selected because some modules are built with
size limitations (and not runtime checking), and --advanced_heap
was not specified.


*******************************************************************************
*** PLACEMENT SUMMARY
***

"A0":  place at 0x800'0000 { ro section .intvec };
"P1":  place in [from 0x800'0000 to 0x801'ffff] { ro };
define block CSTACK with size = 1K, alignment = 8 { };
define block HEAP with size = 512, alignment = 8 { };
"P2":  place in [from 0x2000'0000 to 0x2000'4fff] {
          rw, block CSTACK, block HEAP };
initialize by copy { rw };

  Section            Kind         Address    Size  Object
  -------            ----         -------    ----  ------
"A0":                                        0xec
  .intvec            ro code   0x800'0000    0xec  startup_stm32f103xb.o [1]
                             - 0x800'00ec    0xec

"P1":                                      0x184e
  .text              ro code   0x800'00ec   0x62c  stm32f1xx_hal_rcc.o [1]
  .text              ro code   0x800'0718     0xc  stm32f1xx_hal.o [1]
  .text              ro code   0x800'0724    0x4c  stm32f1xx_hal.o [1]
  .text              ro code   0x800'0770    0x86  ABImemcpy.o [3]
  .text              ro code   0x800'07f6    0x3a  zero_init3.o [3]
  .text              ro code   0x800'0830   0x124  stm32f1xx_hal_cortex.o [1]
  .text              ro code   0x800'0954   0x5c0  stm32f1xx_hal_spi.o [1]
  .text              ro code   0x800'0f14    0xbc  stm32f1xx_hal_msp.o [1]
  .text              ro code   0x800'0fd0     0x6  ABImemclr4.o [3]
  .rodata            const     0x800'0fd6     0x2  stm32f1xx_hal_rcc.o [1]
  .text              ro code   0x800'0fd8   0x278  stm32f1xx_hal_gpio.o [1]
  .text              ro code   0x800'1250    0x32  ABImemset48.o [3]
  .text              ro code   0x800'1284   0x314  enc28j60.o [1]
  .text              ro code   0x800'1598    0x28  stm32f1xx_hal.o [1]
  .text              ro code   0x800'15c0   0x15e  main.o [1]
  .text              ro code   0x800'1720    0x24  stm32f1xx_hal.o [1]
  .text              ro code   0x800'1744    0x2c  copy_init3.o [3]
  .text              ro code   0x800'1770    0x28  data_init.o [3]
  .iar.init_table    const     0x800'1798    0x24  - Linker created -
  .text              ro code   0x800'17bc    0x1e  cmain.o [3]
  .text              ro code   0x800'17da     0x4  low_level_init.o [2]
  .text              ro code   0x800'17de     0x4  exit.o [2]
  .text              ro code   0x800'17e4     0xa  cexit.o [3]
  .text              ro code   0x800'17f0    0x14  exit.o [4]
  Initializer bytes  const     0x800'1804    0x1c  <for P2-1>
  .text              ro code   0x800'1820    0x18  stm32f1xx_hal.o [1]
  .text              ro code   0x800'1838    0x18  stm32f1xx_it.o [1]
  .rodata            const     0x800'1850    0x10  stm32f1xx_hal_rcc.o [1]
  .rodata            const     0x800'1860    0x10  system_stm32f1xx.o [1]
  .text              ro code   0x800'1870    0x10  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1880     0xc  cstartup_M.o [3]
  .text              ro code   0x800'188c     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1890     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1894     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1898     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'189c     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18a0     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18a4     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18a8     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18ac     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18b0     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18b4     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18b8     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18bc     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18c0     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18c4     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18c8     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18cc     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18d0     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18d4     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18d8     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18dc     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18e0     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18e4     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18e8     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18ec     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18f0     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18f4     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18f8     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'18fc     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1900     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1904     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1908     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'190c     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1910     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1914     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1918     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'191c     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1920     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1924     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1928     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'192c     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1930     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1934     0x4  startup_stm32f103xb.o [1]
  .text              ro code   0x800'1938     0x2  system_stm32f1xx.o [1]
  .rodata            const     0x800'193a     0x0  zero_init3.o [3]
  .rodata            const     0x800'193a     0x0  copy_init3.o [3]
                             - 0x800'193a  0x184e

"P2", part 1 of 3:                           0x1c
  P2-1                        0x2000'0000    0x19  <Init block>
    .data            inited   0x2000'0000     0x8  enc28j60.o [1]
    .data            inited   0x2000'0008     0x8  enc28j60.o [1]
    .data            inited   0x2000'0010     0x4  stm32f1xx_hal.o [1]
    .data            inited   0x2000'0014     0x4  system_stm32f1xx.o [1]
    .data            inited   0x2000'0018     0x1  stm32f1xx_hal.o [1]
                            - 0x2000'0019    0x19

"P2", part 2 of 3:                           0x60
  .bss               zero     0x2000'001c    0x58  main.o [1]
  .bss               zero     0x2000'0074     0x4  stm32f1xx_hal.o [1]
  .bss               zero     0x2000'0078     0x1  enc28j60.o [1]
                            - 0x2000'0079    0x5d

"P2", part 3 of 3:                          0x400
  CSTACK                      0x2000'0080   0x400  <Block>
    CSTACK           uninit   0x2000'0080   0x400  <Block tail>
                            - 0x2000'0480   0x400

Unused ranges:

         From           To      Size
         ----           --      ----
   0x800'193a   0x801'ffff  0x1'e6c6
  0x2000'007c  0x2000'007f       0x4
  0x2000'0480  0x2000'4fff    0x4b80


*******************************************************************************
*** INIT TABLE
***

          Address      Size
          -------      ----
Zero (__iar_zero_init3)
    1 destination range, total size 0x5d:
          0x2000'001c  0x5d

Copy (__iar_copy_init3)
    1 source range, total size 0x1c (112% of destination):
           0x800'1804  0x1c
    1 destination range, total size 0x19:
          0x2000'0000  0x19



*******************************************************************************
*** MODULE SUMMARY
***

    Module                  ro code  ro data  rw data
    ------                  -------  -------  -------
command line/config:
    -------------------------------------------------
    Total:

D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj: [1]
    enc28j60.o                  788       16       17
    main.o                      350                88
    startup_stm32f103xb.o       424
    stm32f1xx_hal.o             188        5        9
    stm32f1xx_hal_cortex.o      292
    stm32f1xx_hal_gpio.o        632
    stm32f1xx_hal_msp.o         188
    stm32f1xx_hal_rcc.o       1 580       18
    stm32f1xx_hal_spi.o       1 472
    stm32f1xx_it.o               24
    system_stm32f1xx.o            2       20        4
    -------------------------------------------------
    Total:                    5 940       59      118

dl7M_tln.a: [2]
    exit.o                        4
    low_level_init.o              4
    -------------------------------------------------
    Total:                        8

rt7M_tl.a: [3]
    ABImemclr4.o                  6
    ABImemcpy.o                 134
    ABImemset48.o                50
    cexit.o                      10
    cmain.o                      30
    copy_init3.o                 44
    cstartup_M.o                 12
    data_init.o                  40
    zero_init3.o                 58
    -------------------------------------------------
    Total:                      384

shb_l.a: [4]
    exit.o                       20
    -------------------------------------------------
    Total:                       20

    Gaps                          8
    Linker created                        39    1 024
-----------------------------------------------------
    Grand Total:              6 360       98    1 142


*******************************************************************************
*** ENTRY LIST
***

Entry                       Address   Size  Type      Object
-----                       -------   ----  ----      ------
.iar.init_table$$Base    0x800'1798          --   Gb  - Linker created -
.iar.init_table$$Limit   0x800'17bc          --   Gb  - Linker created -
?main                    0x800'17bd         Code  Gb  cmain.o [3]
AHBPrescTable            0x800'1860   0x10  Data  Gb  system_stm32f1xx.o [1]
BitFieldSet              0x800'1389   0x38  Code  Lc  enc28j60.o [1]
BusFault_Handler         0x800'183f    0x2  Code  Gb  stm32f1xx_it.o [1]
CSTACK$$Base            0x2000'0080          --   Gb  - Linker created -
CSTACK$$Limit           0x2000'0480          --   Gb  - Linker created -
CheckBank                0x800'1313   0x76  Code  Lc  enc28j60.o [1]
DebugMon_Handler         0x800'1845    0x2  Code  Gb  stm32f1xx_it.o [1]
ENC28J60_Init            0x800'14d1   0xb4  Code  Gb  enc28j60.o [1]
ENC28J60_StartReceiving
                         0x800'1495    0xc  Code  Gb  enc28j60.o [1]
Error_Handler            0x800'171d    0x2  Code  Gb  main.o [1]
HAL_Delay                0x800'1599   0x28  Code  Wk  stm32f1xx_hal.o [1]
HAL_GPIO_Init            0x800'0fd9  0x21e  Code  Gb  stm32f1xx_hal_gpio.o [1]
HAL_GPIO_WritePin        0x800'11f7   0x1a  Code  Gb  stm32f1xx_hal_gpio.o [1]
HAL_GetTick              0x800'0719    0xc  Code  Wk  stm32f1xx_hal.o [1]
HAL_IncTick              0x800'1821   0x18  Code  Wk  stm32f1xx_hal.o [1]
HAL_Init                 0x800'1721   0x20  Code  Gb  stm32f1xx_hal.o [1]
HAL_InitTick             0x800'0725   0x4c  Code  Wk  stm32f1xx_hal.o [1]
HAL_MspInit              0x800'0f15   0x3c  Code  Gb  stm32f1xx_hal_msp.o [1]
HAL_NVIC_SetPriority     0x800'0901   0x2a  Code  Gb  stm32f1xx_hal_cortex.o [1]
HAL_NVIC_SetPriorityGrouping
                         0x800'08f5    0xc  Code  Gb  stm32f1xx_hal_cortex.o [1]
HAL_RCC_ClockConfig      0x800'04ed  0x14e  Code  Gb  stm32f1xx_hal_rcc.o [1]
HAL_RCC_GetSysClockFreq
                         0x800'063b   0x70  Code  Gb  stm32f1xx_hal_rcc.o [1]
HAL_RCC_OscConfig        0x800'00ed  0x400  Code  Gb  stm32f1xx_hal_rcc.o [1]
HAL_SPI_Init             0x800'0955   0xc4  Code  Gb  stm32f1xx_hal_spi.o [1]
HAL_SPI_MspInit          0x800'0f51   0x6a  Code  Gb  stm32f1xx_hal_msp.o [1]
HAL_SPI_Transmit         0x800'0a19  0x1b6  Code  Gb  stm32f1xx_hal_spi.o [1]
HAL_SPI_TransmitReceive
                         0x800'0bcf  0x23c  Code  Gb  stm32f1xx_hal_spi.o [1]
HAL_SYSTICK_Config       0x800'092b    0xc  Code  Gb  stm32f1xx_hal_cortex.o [1]
HardFault_Handler        0x800'183b    0x2  Code  Gb  stm32f1xx_it.o [1]
MX_GPIO_Init             0x800'1689   0x84  Code  Lc  main.o [1]
MX_SPI1_Init             0x800'1643   0x46  Code  Lc  main.o [1]
MemManage_Handler        0x800'183d    0x2  Code  Gb  stm32f1xx_it.o [1]
NMI_Handler              0x800'1839    0x2  Code  Gb  stm32f1xx_it.o [1]
NVIC_EncodePriority      0x800'0885   0x40  Code  Lc  stm32f1xx_hal_cortex.o [1]
PendSV_Handler           0x800'1847    0x2  Code  Gb  stm32f1xx_it.o [1]
RCC_Delay                0x800'06ab   0x26  Code  Lc  stm32f1xx_hal_rcc.o [1]
ReadByte                 0x800'12ab   0x2a  Code  Lc  enc28j60.o [1]
ReadControlReg           0x800'13c1   0x54  Code  Lc  enc28j60.o [1]
Region$$Table$$Base      0x800'1798          --   Gb  - Linker created -
Region$$Table$$Limit     0x800'17bc          --   Gb  - Linker created -
SPI_EndRxTxTransaction   0x800'0ee5   0x2a  Code  Lc  stm32f1xx_hal_spi.o [1]
SPI_WaitFlagStateUntilTimeout
                         0x800'0e0b   0xda  Code  Lc  stm32f1xx_hal_spi.o [1]
SVC_Handler              0x800'1843    0x2  Code  Gb  stm32f1xx_it.o [1]
SetCS                    0x800'1285   0x14  Code  Lc  enc28j60.o [1]
SysTick_Config           0x800'08c5   0x30  Code  Lc  stm32f1xx_hal_cortex.o [1]
SysTick_Handler          0x800'1849    0x8  Code  Gb  stm32f1xx_it.o [1]
SystemClock_Config       0x800'15d9   0x6a  Code  Gb  main.o [1]
SystemCoreClock         0x2000'0014    0x4  Data  Gb  system_stm32f1xx.o [1]
SystemInit               0x800'1939    0x2  Code  Gb  system_stm32f1xx.o [1]
SystemReset              0x800'1471   0x24  Code  Lc  enc28j60.o [1]
UsageFault_Handler       0x800'1841    0x2  Code  Gb  stm32f1xx_it.o [1]
WriteByte                0x800'1299   0x12  Code  Lc  enc28j60.o [1]
WriteCommand             0x800'12f5   0x1e  Code  Lc  enc28j60.o [1]
WriteControlReg          0x800'1415   0x38  Code  Lc  enc28j60.o [1]
WriteControlRegPair      0x800'144d   0x24  Code  Lc  enc28j60.o [1]
WritePhyReg              0x800'14a1   0x30  Code  Lc  enc28j60.o [1]
__NVIC_GetPriorityGrouping
                         0x800'084f    0xa  Code  Lc  stm32f1xx_hal_cortex.o [1]
__NVIC_SetPriority       0x800'0859   0x2c  Code  Lc  stm32f1xx_hal_cortex.o [1]
__NVIC_SetPriorityGrouping
                         0x800'0831   0x1e  Code  Lc  stm32f1xx_hal_cortex.o [1]
__aeabi_memclr4          0x800'0fd1         Code  Gb  ABImemclr4.o [3]
__aeabi_memcpy4          0x800'0771         Code  Gb  ABImemcpy.o [3]
__aeabi_memcpy8          0x800'0771         Code  Gb  ABImemcpy.o [3]
__cmain                  0x800'17bd         Code  Gb  cmain.o [3]
__exit                   0x800'17f1   0x14  Code  Gb  exit.o [4]
__iar_Memset4_word       0x800'1251         Code  Gb  ABImemset48.o [3]
__iar_Memset8_word       0x800'1251         Code  Gb  ABImemset48.o [3]
__iar_copy_init3         0x800'1745   0x2c  Code  Gb  copy_init3.o [3]
__iar_data_init3         0x800'1771   0x28  Code  Gb  data_init.o [3]
__iar_program_start      0x800'1881         Code  Gb  cstartup_M.o [3]
__iar_zero_init3         0x800'07f7   0x3a  Code  Gb  zero_init3.o [3]
__low_level_init         0x800'17db    0x4  Code  Gb  low_level_init.o [2]
__vector_table           0x800'0000         Data  Gb  startup_stm32f103xb.o [1]
_call_main               0x800'17c9         Code  Gb  cmain.o [3]
_exit                    0x800'17e5         Code  Gb  cexit.o [3]
_main                    0x800'17d7         Code  Gb  cmain.o [3]
commandOpCodes          0x2000'0008    0x8  Data  Lc  enc28j60.o [1]
curBank                 0x2000'0078    0x1  Data  Lc  enc28j60.o [1]
exit                     0x800'17df    0x4  Code  Gb  exit.o [2]
getRegAddr               0x800'12eb    0xa  Code  Lc  enc28j60.o [1]
getRegBank               0x800'12e1    0xa  Code  Lc  enc28j60.o [1]
getRegType               0x800'12d5    0xc  Code  Lc  enc28j60.o [1]
hspi1                   0x2000'001c   0x58  Data  Gb  main.o [1]
macAddr                 0x2000'0000    0x8  Data  Gb  enc28j60.o [1]
main                     0x800'15c1   0x18  Code  Gb  main.o [1]
uwTick                  0x2000'0074    0x4  Data  Gb  stm32f1xx_hal.o [1]
uwTickFreq              0x2000'0018    0x1  Data  Gb  stm32f1xx_hal.o [1]
uwTickPrio              0x2000'0010    0x4  Data  Gb  stm32f1xx_hal.o [1]


[1] = D:\Projects\MicroTechnics\Projects_site\MT_ENC28J60_Part_2\EWARM\MT_ENC28J60\Obj
[2] = dl7M_tln.a
[3] = rt7M_tl.a
[4] = shb_l.a

  6 360 bytes of readonly  code memory
     98 bytes of readonly  data memory
  1 142 bytes of readwrite data memory

Errors: none
Warnings: none
