###############################################################################
#
# IAR ELF Linker V7.50.2.10312/W32 for ARM                12/Aug/2020  22:37:19
# Copyright 2007-2015 IAR Systems AB.
#
#    Output file  =  
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Exe\MT_Encoder_AS5048.out
#    Map file     =  
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\List\MT_Encoder_AS5048.map
#    Command line =  
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\main.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\startup_stm32f103xb.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_cortex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_dma.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_exti.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_flash.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_flash_ex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_gpio.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_gpio_ex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_msp.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_pwr.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_rcc.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_rcc_ex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_tim.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_hal_tim_ex.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\stm32f1xx_it.o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj\system_stm32f1xx.o
#        --redirect _Printf=_PrintfFull --redirect _Scanf=_ScanfFull -o
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Exe\MT_Encoder_AS5048.out
#        --map
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\List\MT_Encoder_AS5048.map
#        --config
#        D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM/stm32f103xb_flash.icf
#        --semihosting --entry __iar_program_start --vfe
#
###############################################################################

*******************************************************************************
*** RUNTIME MODEL ATTRIBUTES
***

CppFlavor       = *
__SystemLibrary = DLib


*******************************************************************************
*** PLACEMENT SUMMARY
***

"A1":  place at 0x08000000 { ro section .intvec };
"P1":  place in [from 0x08000000 to 0x0801ffff] { ro };
"P2":  place in [from 0x20000000 to 0x20004fff] { rw, block CSTACK, block HEAP };

  Section            Kind        Address    Size  Object
  -------            ----        -------    ----  ------
"A1":                                       0xec
  .intvec            ro code  0x08000000    0xec  startup_stm32f103xb.o [1]
                            - 0x080000ec    0xec

"P1":                                     0x1a8c
  .text              ro code  0x080000ec   0x6d0  stm32f1xx_hal_rcc.o [1]
  .text              ro code  0x080007bc    0x8c  stm32f1xx_hal.o [1]
  .text              ro code  0x08000848    0x56  ABImemcpy_unaligned.o [5]
  .rodata            const    0x0800089e     0x2  stm32f1xx_hal_rcc.o [1]
  .text              ro code  0x080008a0   0x144  stm32f1xx_hal_cortex.o [1]
  .text              ro code  0x080009e4    0xc8  stm32f1xx_hal_msp.o [1]
  .text              ro code  0x08000aac     0x6  ABImemclr4.o [5]
  .text              ro code  0x08000ab4   0x2f8  stm32f1xx_hal_gpio.o [1]
  .text              ro code  0x08000dac    0x32  ABImemset48.o [5]
  .text              ro code  0x08000de0   0x68a  stm32f1xx_hal_tim.o [1]
  .text              ro code  0x0800146c   0x23a  main.o [1]
  .text              ro code  0x080016a8    0x56  stm32f1xx_hal_tim_ex.o [1]
  .text              ro code  0x08001700    0x1e  I32ToFlt.o [4]
  .text              ro code  0x08001720    0xfc  FltDiv.o [4]
  .text              ro code  0x0800181c    0xd8  FltMul.o [4]
  .text              ro code  0x080018f4    0x68  system_stm32f1xx.o [1]
  .text              ro code  0x0800195c    0x40  zero_init3.o [5]
  .text              ro code  0x0800199c    0x2c  copy_init3.o [5]
  .text              ro code  0x080019c8    0x28  stm32f1xx_it.o [1]
  .text              ro code  0x080019f0    0x28  data_init.o [5]
  .iar.init_table    const    0x08001a18    0x24  - Linker created -
  .text              ro code  0x08001a3c    0x1a  cmain.o [5]
  .text              ro code  0x08001a56     0x4  low_level_init.o [3]
  .text              ro code  0x08001a5a     0x4  exit.o [3]
  .text              ro code  0x08001a60     0xa  cexit.o [5]
  .text              ro code  0x08001a6c    0x14  exit.o [6]
  .rodata            const    0x08001a80    0x10  stm32f1xx_hal_rcc.o [1]
  .rodata            const    0x08001a90    0x10  system_stm32f1xx.o [1]
  .text              ro code  0x08001aa0    0x10  startup_stm32f103xb.o [1]
  .text              ro code  0x08001ab0     0xc  cstartup_M.o [5]
  Initializer bytes  const    0x08001abc     0xc  <for P2-1>
  .rodata            const    0x08001ac8     0x8  main.o [1]
  .text              ro code  0x08001ad0     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001ad4     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001ad8     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001adc     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001ae0     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001ae4     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001ae8     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001aec     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001af0     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001af4     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001af8     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001afc     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b00     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b04     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b08     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b0c     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b10     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b14     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b18     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b1c     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b20     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b24     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b28     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b2c     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b30     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b34     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b38     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b3c     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b40     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b44     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b48     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b4c     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b50     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b54     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b58     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b5c     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b60     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b64     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b68     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b6c     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b70     0x4  startup_stm32f103xb.o [1]
  .text              ro code  0x08001b74     0x4  startup_stm32f103xb.o [1]
  .rodata            const    0x08001b78     0x0  zero_init3.o [5]
  .rodata            const    0x08001b78     0x0  copy_init3.o [5]
                            - 0x08001b78  0x1a8c

"P2", part 1 of 3:                           0xc
  P2-1                        0x20000000     0x9  <Init block>
    .data            inited   0x20000000     0x4  stm32f1xx_hal.o [1]
    .data            inited   0x20000004     0x4  system_stm32f1xx.o [1]
    .data            inited   0x20000008     0x1  stm32f1xx_hal.o [1]
                            - 0x20000009     0x9

"P2", part 2 of 3:                         0x400
  CSTACK                      0x20000010   0x400  <Block>
    CSTACK           uninit   0x20000010   0x400  <Block tail>
                            - 0x20000410   0x400

"P2", part 3 of 3:                          0x50
  .bss               zero     0x20000410    0x40  main.o [1]
  .bss               zero     0x20000450     0x4  main.o [1]
  .bss               zero     0x20000454     0x4  main.o [1]
  .bss               zero     0x20000458     0x4  main.o [1]
  .bss               zero     0x2000045c     0x4  stm32f1xx_hal.o [1]
                            - 0x20000460    0x50


*******************************************************************************
*** INIT TABLE
***

          Address     Size
          -------     ----
Zero (__iar_zero_init3)
    1 destination range, total size 0x50:
          0x20000410  0x50

Copy (__iar_copy_init3)
    1 source range, total size 0xc (133% of destination):
          0x08001abc   0xc
    1 destination range, total size 0x9:
          0x20000000   0x9



*******************************************************************************
*** MODULE SUMMARY
***

    Module                  ro code  ro data  rw data
    ------                  -------  -------  -------
D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj: [1]
    main.o                      570        8       76
    startup_stm32f103xb.o       420
    stm32f1xx_hal.o             140        5        9
    stm32f1xx_hal_cortex.o      324
    stm32f1xx_hal_gpio.o        760
    stm32f1xx_hal_msp.o         200
    stm32f1xx_hal_rcc.o       1 744       18
    stm32f1xx_hal_tim.o       1 674
    stm32f1xx_hal_tim_ex.o       86
    stm32f1xx_it.o               40
    system_stm32f1xx.o          104       20        4
    -------------------------------------------------
    Total:                    6 062       51       89

command line: [2]
    -------------------------------------------------
    Total:

dl7M_tln.a: [3]
    exit.o                        4
    low_level_init.o              4
    -------------------------------------------------
    Total:                        8

m7M_tl.a: [4]
    FltDiv.o                    252
    FltMul.o                    216
    I32ToFlt.o                   30
    -------------------------------------------------
    Total:                      498

rt7M_tl.a: [5]
    ABImemclr4.o                  6
    ABImemcpy_unaligned.o        86
    ABImemset48.o                50
    cexit.o                      10
    cmain.o                      26
    copy_init3.o                 44
    cstartup_M.o                 12
    data_init.o                  40
    zero_init3.o                 64
    -------------------------------------------------
    Total:                      338

shb_l.a: [6]
    exit.o                       20
    -------------------------------------------------
    Total:                       20

    Gaps                         16
    Linker created                        39    1 024
-----------------------------------------------------
    Grand Total:              6 942       90    1 113


*******************************************************************************
*** ENTRY LIST
***

Entry                      Address   Size  Type      Object
-----                      -------   ----  ----      ------
.iar.init_table$$Base   0x08001a18          --   Gb  - Linker created -
.iar.init_table$$Limit  0x08001a3c          --   Gb  - Linker created -
?main                   0x08001a3d         Code  Gb  cmain.o [5]
AHBPrescTable           0x08001a90   0x10  Data  Gb  system_stm32f1xx.o [1]
BusFault_Handler        0x080019cf    0x2  Code  Gb  stm32f1xx_it.o [1]
CSTACK$$Base            0x20000010          --   Gb  - Linker created -
CSTACK$$Limit           0x20000410          --   Gb  - Linker created -
DebugMon_Handler        0x080019d5    0x2  Code  Gb  stm32f1xx_it.o [1]
Error_Handler           0x080016a5    0x2  Code  Gb  main.o [1]
HAL_GPIO_Init           0x08000ab5  0x2b6  Code  Gb  stm32f1xx_hal_gpio.o [1]
HAL_GetTick             0x0800082f    0x6  Code  Wk  stm32f1xx_hal.o [1]
HAL_IncTick             0x0800081f   0x10  Code  Wk  stm32f1xx_hal.o [1]
HAL_Init                0x080007bd   0x22  Code  Gb  stm32f1xx_hal.o [1]
HAL_InitTick            0x080007df   0x40  Code  Wk  stm32f1xx_hal.o [1]
HAL_MspInit             0x080009e5   0x48  Code  Gb  stm32f1xx_hal_msp.o [1]
HAL_NVIC_EnableIRQ      0x080009a9    0xe  Code  Gb  stm32f1xx_hal_cortex.o [1]
HAL_NVIC_SetPriority    0x08000983   0x26  Code  Gb  stm32f1xx_hal_cortex.o [1]
HAL_NVIC_SetPriorityGrouping
                        0x08000977    0xc  Code  Gb  stm32f1xx_hal_cortex.o [1]
HAL_RCC_ClockConfig     0x0800056d  0x16e  Code  Gb  stm32f1xx_hal_rcc.o [1]
HAL_RCC_GetSysClockFreq
                        0x080006db   0x78  Code  Gb  stm32f1xx_hal_rcc.o [1]
HAL_RCC_OscConfig       0x080000ed  0x480  Code  Gb  stm32f1xx_hal_rcc.o [1]
HAL_SYSTICK_Config      0x080009b7    0xc  Code  Gb  stm32f1xx_hal_cortex.o [1]
HAL_TIMEx_BreakCallback
                        0x080016fd    0x2  Code  Wk  stm32f1xx_hal_tim_ex.o [1]
HAL_TIMEx_CommutCallback
                        0x080016fb    0x2  Code  Wk  stm32f1xx_hal_tim_ex.o [1]
HAL_TIMEx_MasterConfigSynchronization
                        0x080016a9   0x52  Code  Gb  stm32f1xx_hal_tim_ex.o [1]
HAL_TIM_Base_Init       0x08000de1   0x38  Code  Gb  stm32f1xx_hal_tim.o [1]
HAL_TIM_Base_MspInit    0x08000a2d   0x6e  Code  Gb  stm32f1xx_hal_msp.o [1]
HAL_TIM_ConfigClockSource
                        0x08001119   0xee  Code  Gb  stm32f1xx_hal_tim.o [1]
HAL_TIM_IC_CaptureCallback
                        0x08001605   0x7a  Code  Gb  main.o [1]
HAL_TIM_IC_ConfigChannel
                        0x08001043   0xd6  Code  Gb  stm32f1xx_hal_tim.o [1]
HAL_TIM_IC_Init         0x08000e19   0x38  Code  Gb  stm32f1xx_hal_tim.o [1]
HAL_TIM_IC_MspInit      0x08000e51    0x2  Code  Wk  stm32f1xx_hal_tim.o [1]
HAL_TIM_IC_Start_IT     0x08000e53   0x7a  Code  Gb  stm32f1xx_hal_tim.o [1]
HAL_TIM_IRQHandler      0x08000ecd  0x176  Code  Gb  stm32f1xx_hal_tim.o [1]
HAL_TIM_OC_DelayElapsedCallback
                        0x08001243    0x2  Code  Wk  stm32f1xx_hal_tim.o [1]
HAL_TIM_PWM_PulseFinishedCallback
                        0x08001245    0x2  Code  Wk  stm32f1xx_hal_tim.o [1]
HAL_TIM_PeriodElapsedCallback
                        0x08001241    0x2  Code  Wk  stm32f1xx_hal_tim.o [1]
HAL_TIM_ReadCapturedValue
                        0x08001207   0x3a  Code  Gb  stm32f1xx_hal_tim.o [1]
HAL_TIM_TriggerCallback
                        0x08001247    0x2  Code  Wk  stm32f1xx_hal_tim.o [1]
HardFault_Handler       0x080019cb    0x2  Code  Gb  stm32f1xx_it.o [1]
MX_GPIO_Init            0x080015cf   0x36  Code  Lc  main.o [1]
MX_TIM2_Init            0x080014ff   0xd0  Code  Lc  main.o [1]
MemManage_Handler       0x080019cd    0x2  Code  Gb  stm32f1xx_it.o [1]
NMI_Handler             0x080019c9    0x2  Code  Gb  stm32f1xx_it.o [1]
NVIC_EncodePriority     0x08000909   0x3e  Code  Lc  stm32f1xx_hal_cortex.o [1]
PendSV_Handler          0x080019d7    0x2  Code  Gb  stm32f1xx_it.o [1]
RCC_Delay               0x08000753   0x26  Code  Lc  stm32f1xx_hal_rcc.o [1]
Region$$Table$$Base     0x08001a18          --   Gb  - Linker created -
Region$$Table$$Limit    0x08001a3c          --   Gb  - Linker created -
SVC_Handler             0x080019d3    0x2  Code  Gb  stm32f1xx_it.o [1]
SysTick_Config          0x08000947   0x30  Code  Lc  stm32f1xx_hal_cortex.o [1]
SysTick_Handler         0x080019d9    0x8  Code  Gb  stm32f1xx_it.o [1]
SystemClock_Config      0x08001491   0x6e  Code  Gb  main.o [1]
SystemCoreClock         0x20000004    0x4  Data  Gb  system_stm32f1xx.o [1]
SystemInit              0x080018f5   0x4e  Code  Gb  system_stm32f1xx.o [1]
TIM2_IRQHandler         0x080019e1    0xa  Code  Gb  stm32f1xx_it.o [1]
TIM_Base_SetConfig      0x08001249   0x66  Code  Gb  stm32f1xx_hal_tim.o [1]
TIM_CCxChannelCmd       0x08001447   0x24  Code  Gb  stm32f1xx_hal_tim.o [1]
TIM_ETR_SetConfig       0x0800142d   0x1a  Code  Gb  stm32f1xx_hal_tim.o [1]
TIM_ITRx_SetConfig      0x0800141b   0x12  Code  Lc  stm32f1xx_hal_tim.o [1]
TIM_TI1_ConfigInputStage
                        0x0800131d   0x28  Code  Lc  stm32f1xx_hal_tim.o [1]
TIM_TI1_SetConfig       0x080012af   0x60  Code  Gb  stm32f1xx_hal_tim.o [1]
TIM_TI2_ConfigInputStage
                        0x0800137f   0x2a  Code  Lc  stm32f1xx_hal_tim.o [1]
TIM_TI2_SetConfig       0x08001345   0x3a  Code  Lc  stm32f1xx_hal_tim.o [1]
TIM_TI3_SetConfig       0x080013a9   0x38  Code  Lc  stm32f1xx_hal_tim.o [1]
TIM_TI4_SetConfig       0x080013e1   0x3a  Code  Lc  stm32f1xx_hal_tim.o [1]
UsageFault_Handler      0x080019d1    0x2  Code  Gb  stm32f1xx_it.o [1]
__NVIC_EnableIRQ        0x080008c9   0x1a  Code  Lc  stm32f1xx_hal_cortex.o [1]
__NVIC_GetPriorityGrouping
                        0x080008bf    0xa  Code  Lc  stm32f1xx_hal_cortex.o [1]
__NVIC_SetPriority      0x080008e3   0x26  Code  Lc  stm32f1xx_hal_cortex.o [1]
__NVIC_SetPriorityGrouping
                        0x080008a1   0x1e  Code  Lc  stm32f1xx_hal_cortex.o [1]
__aeabi_fdiv            0x08001721         Code  Gb  FltDiv.o [4]
__aeabi_fmul            0x0800181d         Code  Gb  FltMul.o [4]
__aeabi_memclr4         0x08000aad         Code  Gb  ABImemclr4.o [5]
__aeabi_ui2f            0x08001701         Code  Gb  I32ToFlt.o [4]
__cmain                 0x08001a3d         Code  Gb  cmain.o [5]
__exit                  0x08001a6d   0x14  Code  Gb  exit.o [6]
__iar_Memset4_word      0x08000dad         Code  Gb  ABImemset48.o [5]
__iar_Memset8_word      0x08000dad         Code  Gb  ABImemset48.o [5]
__iar_copy_init3        0x0800199d   0x2c  Code  Gb  copy_init3.o [5]
__iar_data_init3        0x080019f1   0x28  Code  Gb  data_init.o [5]
__iar_program_start     0x08001ab1         Code  Gb  cstartup_M.o [5]
__iar_ui2f              0x08001705         Code  Gb  I32ToFlt.o [4]
__iar_unaligned___aeabi_memcpy4
                        0x08000849         Code  Gb  ABImemcpy_unaligned.o [5]
__iar_unaligned___aeabi_memcpy8
                        0x08000849         Code  Gb  ABImemcpy_unaligned.o [5]
__iar_zero_init3        0x0800195d   0x40  Code  Gb  zero_init3.o [5]
__low_level_init        0x08001a57    0x4  Code  Gb  low_level_init.o [3]
__vector_table          0x08000000         Data  Gb  startup_stm32f103xb.o [1]
_call_main              0x08001a49         Code  Gb  cmain.o [5]
_exit                   0x08001a61         Code  Gb  cexit.o [5]
_main                   0x08001a53         Code  Gb  cmain.o [5]
angle                   0x20000458    0x4  Data  Gb  main.o [1]
exit                    0x08001a5b    0x4  Code  Gb  exit.o [3]
htim2                   0x20000410   0x40  Data  Gb  main.o [1]
main                    0x0800146d   0x24  Code  Gb  main.o [1]
period                  0x20000450    0x4  Data  Gb  main.o [1]
pulseWidth              0x20000454    0x4  Data  Gb  main.o [1]
uwTick                  0x2000045c    0x4  Data  Gb  stm32f1xx_hal.o [1]
uwTickFreq              0x20000008    0x1  Data  Gb  stm32f1xx_hal.o [1]
uwTickPrio              0x20000000    0x4  Data  Gb  stm32f1xx_hal.o [1]


[1] = D:\Projects\MicroTechnics\Projects_site\MT_Encoder_AS5048\EWARM\MT_Encoder_AS5048\Obj
[2] = command line
[3] = dl7M_tln.a
[4] = m7M_tl.a
[5] = rt7M_tl.a
[6] = shb_l.a

  6 942 bytes of readonly  code memory
     90 bytes of readonly  data memory
  1 113 bytes of readwrite data memory

Errors: none
Warnings: none
