#MicroXplorer Configuration settings - do not modify
#Fri Oct 02 16:13:35 MSK 2015
File.Version=5
KeepUserPlacement=false
Mcu.Family=STM32F1
Mcu.IP0=FATFS
Mcu.IP1=NVIC
Mcu.IP2=RCC
Mcu.IP3=SDIO
Mcu.IPNb=4
Mcu.Name=STM32F103V(C-D-E)Tx
Mcu.Package=LQFP100
Mcu.Pin0=PC8
Mcu.Pin1=PC9
Mcu.Pin2=PC10
Mcu.Pin3=PC11
Mcu.Pin4=PC12
Mcu.Pin5=PD2
Mcu.Pin6=VP_FATFS_VS_SDIO
Mcu.PinsNb=7
Mcu.UserName=STM32F103VETx
MxCube.Version=4.6.0
MxDb.Version=DB.4.0.60
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SysTick_IRQn=true\:0\:0\:false
PC10.Mode=SD_4_bits_Wide_bus
PC10.Signal=SDIO_D2
PC11.Mode=SD_4_bits_Wide_bus
PC11.Signal=SDIO_D3
PC12.Mode=SD_4_bits_Wide_bus
PC12.Signal=SDIO_CK
PC8.Mode=SD_4_bits_Wide_bus
PC8.Signal=SDIO_D0
PC9.Mode=SD_4_bits_Wide_bus
PC9.Signal=SDIO_D1
PCC.Family=STM32F1
PCC.MCU=STM32F103V(C-D-E)Tx
PCC.MXVersion=4.6.0
PCC.PartNumber=STM32F103VETx
PCC.Seq0=0
PCC.SubFamily=STM32F103
PCC.Temperature=25
PCC.Vdd=3.3
PD2.Mode=SD_4_bits_Wide_bus
PD2.Signal=SDIO_CMD
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=2
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F103VETx
ProjectManager.FirmwarePackage=STM32Cube FW_F1 V1.0.0
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=0
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=STM32Cube_SDCardProject.ioc
ProjectManager.ProjectName=STM32Cube_SDCardProject
ProjectManager.TargetToolchain=EWARM 6.70
ProjectManager.ToolChainLocation=
RCC.ADCFreqValue=4000000
RCC.AHBFreq_Value=8000000
RCC.APB1CLKDivider=RCC_HCLK_DIV2
RCC.APB1Freq_Value=4000000
RCC.APB1TimFreq_Value=8000000
RCC.APB2Freq_Value=8000000
RCC.APB2TimFreq_Value=8000000
RCC.FCLKCortexFreq_Value=8000000
RCC.FSMCFreq_Value=8000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=8000000
RCC.I2S2Freq_Value=8000000
RCC.I2S3Freq_Value=8000000
RCC.IPParameters=HCLKFreq_Value,SYSCLKFreq_VALUE,PLLCLKFreq_Value,FamilyName,SDIOFreq_Value,USBFreq_Value,PLLMCOFreq_Value,APB1CLKDivider,FCLKCortexFreq_Value,APB2Freq_Value,APB2TimFreq_Value,VCOOutput2Freq_Value,MCOFreq_Value,I2S3Freq_Value,ADCFreqValue,I2S2Freq_Value,SDIOHCLKDiv2FreqValue,FSMCFreq_Value,APB1TimFreq_Value,APB1Freq_Value,AHBFreq_Value,TimSysFreq_Value
RCC.MCOFreq_Value=8000000
RCC.PLLCLKFreq_Value=8000000
RCC.PLLMCOFreq_Value=4000000
RCC.SDIOFreq_Value=8000000
RCC.SDIOHCLKDiv2FreqValue=4000000
RCC.SYSCLKFreq_VALUE=8000000
RCC.TimSysFreq_Value=1000000
RCC.USBFreq_Value=8000000
RCC.VCOOutput2Freq_Value=4000000
SDIO.BusWide-SD_4_bits_Wide_bus=SDIO_BUS_WIDE_1B
SDIO.ClockDiv-SD_4_bits_Wide_bus=3
SDIO.IPParameters=BusWide-SD_4_bits_Wide_bus,ClockDiv-SD_4_bits_Wide_bus,WideMode
SDIO.WideMode=SDIO_BUS_WIDE_4B
VP_FATFS_VS_SDIO.Mode=SDIO
VP_FATFS_VS_SDIO.Signal=FATFS_VS_SDIO
