Static Call Graph - [lin_m_s\lin_m_s.axf]

# Static Call Graph for image lin_m_s\lin_m_s.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Sun Dec 19 11:50:21 2021

### Maximum Stack Usage = 248 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl

### Mutually Recursive functions

- ADC1_COMP_IRQHandler ⇒ ADC1_COMP_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- NMI_Handler ⇒ NMI_Handler

  ### Function Pointers

  - ADC1_COMP_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - CEC_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - DMA1_Channel2_3_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - DMA1_Channel4_5_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - EXTI0_1_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - EXTI2_3_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - EXTI4_15_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - FLASH_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - HardFault_Handler from stm32f0xx_it.o(i.HardFault_Handler) referenced from startup_stm32f051x8.o(RESET)
  - I2C1_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - I2C2_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - NMI_Handler from stm32f0xx_it.o(i.NMI_Handler) referenced from startup_stm32f051x8.o(RESET)
  - PVD_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - PendSV_Handler from stm32f0xx_it.o(i.PendSV_Handler) referenced from startup_stm32f051x8.o(RESET)
  - RCC_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - RTC_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - Reset_Handler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - SPI1_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - SPI2_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - SVC_Handler from stm32f0xx_it.o(i.SVC_Handler) referenced from startup_stm32f051x8.o(RESET)
  - SysTick_Handler from stm32f0xx_it.o(i.SysTick_Handler) referenced from startup_stm32f051x8.o(RESET)
  - SystemInit from system_stm32f0xx.o(i.SystemInit) referenced from startup_stm32f051x8.o(.text)
  - TIM14_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - TIM15_IRQHandler from stm32f0xx_it.o(i.TIM15_IRQHandler) referenced from startup_stm32f051x8.o(RESET)
  - TIM16_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - TIM17_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - TIM1_BRK_UP_TRG_COM_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - TIM2_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - TIM3_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - TSC_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - UART_DMAAbortOnError from stm32f0xx_hal_uart.o(i.UART_DMAAbortOnError) referenced from stm32f0xx_hal_uart.o(i.HAL_UART_IRQHandler)
  - UART_RxISR_16BIT from stm32f0xx_hal_uart.o(i.UART_RxISR_16BIT) referenced from stm32f0xx_hal_uart.o(i.UART_Start_Receive_IT)
  - UART_RxISR_8BIT from stm32f0xx_hal_uart.o(i.UART_RxISR_8BIT) referenced from stm32f0xx_hal_uart.o(i.UART_Start_Receive_IT)
  - UART_TxISR_16BIT from stm32f0xx_hal_uart.o(i.UART_TxISR_16BIT) referenced from stm32f0xx_hal_uart.o(i.HAL_UART_Transmit_IT)
  - UART_TxISR_8BIT from stm32f0xx_hal_uart.o(i.UART_TxISR_8BIT) referenced from stm32f0xx_hal_uart.o(i.HAL_UART_Transmit_IT)
  - USART1_IRQHandler from stm32f0xx_it.o(i.USART1_IRQHandler) referenced from startup_stm32f051x8.o(RESET)
  - USART2_IRQHandler from stm32f0xx_it.o(i.USART2_IRQHandler) referenced from startup_stm32f051x8.o(RESET)
  - WWDG_IRQHandler from startup_stm32f051x8.o(.text) referenced from startup_stm32f051x8.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f051x8.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  ADC1_COMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Calls]

  - >> ADC1_COMP_IRQHandler
  [Called By]
  - >> ADC1_COMP_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f051x8.o(RESET)

  CEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  DMA1_Channel2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  DMA1_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  EXTI0_1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  EXTI2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  EXTI4_15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TIM1_BRK_UP_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  TSC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f051x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_uidivmod
  [Called By]
  - >> LIN_Init
  - >> UART_SetConfig
  - >> HAL_InitTick

  __aeabi_uldivmod (Thumb, 96 bytes, Stack size 48 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> __aeabi_llsl
  - >> __aeabi_llsr
  [Called By]
  - >> HAL_RCC_GetSysClockFreq

  __aeabi_llsr (Thumb, 34 bytes, Stack size 8 bytes, llushr.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_llsr
  [Called By]
  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 8 bytes, llushr.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> HAL_UART_MspInit
  - >> SystemClock_Config
  - >> MX_GPIO_Init
  - >> LIN_WriteTxPortState

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_llsl (Thumb, 32 bytes, Stack size 8 bytes, llshl.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_llsl
  [Called By]
  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 8 bytes, llshl.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  HAL_DMA_Abort (Thumb, 68 bytes, Stack size 8 bytes, stm32f0xx_hal_dma.o(i.HAL_DMA_Abort))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA_Abort
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> HAL_UART_AbortReceive

  HAL_DMA_Abort_IT (Thumb, 72 bytes, Stack size 16 bytes, stm32f0xx_hal_dma.o(i.HAL_DMA_Abort_IT))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_DMA_GetError (Thumb, 4 bytes, Stack size 0 bytes, stm32f0xx_hal_dma.o(i.HAL_DMA_GetError))
  [Called By]

  - >> HAL_UART_AbortReceive

  HAL_Delay (Thumb, 32 bytes, Stack size 16 bytes, stm32f0xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> main

  HAL_GPIO_DeInit (Thumb, 186 bytes, Stack size 20 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_DeInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_GPIO_DeInit
  [Called By]
  - >> LIN_WriteTxPortState

  HAL_GPIO_Init (Thumb, 318 bytes, Stack size 24 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> MX_GPIO_Init
  - >> LIN_WriteTxPortState

  HAL_GPIO_ReadPin (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> LIN_ReadRxPortState

  HAL_GPIO_TogglePin (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_TogglePin))
  [Called By]

  - >> LIN_SlaveIdRxCallback

  HAL_GPIO_WritePin (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> MX_GPIO_Init
  - >> LIN_WriteTxPortState

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_Delay
  - >> UART_WaitOnFlagUntilTimeout
  - >> UART_CheckIdleState

  HAL_IncTick (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_MspInit
  - >> HAL_InitTick
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 62 bytes, Stack size 16 bytes, stm32f0xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_InitTick ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  - >> __aeabi_uidivmod
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_LIN_Init (Thumb, 160 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.HAL_LIN_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = HAL_LIN_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_LIN_SendBreak (Thumb, 48 bytes, Stack size 4 bytes, stm32f0xx_hal_uart.o(i.HAL_LIN_SendBreak))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_LIN_SendBreak
  [Called By]
  - >> main

  HAL_MspInit (Thumb, 34 bytes, Stack size 8 bytes, stm32f0xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_MspInit
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_UART_MspInit
  - >> HAL_TIM_Base_MspInit

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Called By]

  - >> HAL_UART_MspInit
  - >> HAL_TIM_Base_MspInit
  - >> HAL_InitTick

  HAL_RCCEx_PeriphCLKConfig (Thumb, 256 bytes, Stack size 24 bytes, stm32f0xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_ClockConfig (Thumb, 278 bytes, Stack size 24 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 128
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> HAL_InitTick
  - >> HAL_GetTick
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> HAL_RCC_GetPCLK1Freq

  HAL_RCC_GetPCLK1Freq (Thumb, 22 bytes, Stack size 4 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK1Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 114 bytes, Stack size 48 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> __ARM_common_ll_muluu
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> UART_SetConfig

  HAL_RCC_OscConfig (Thumb, 1158 bytes, Stack size 32 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_Config (Thumb, 46 bytes, Stack size 4 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_SYSTICK_Config
  [Called By]
  - >> HAL_InitTick

  HAL_TIMEx_BreakCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_CommutCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim_ex.o(i.HAL_TIMEx_CommutCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 88 bytes, Stack size 16 bytes, stm32f0xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM15_Init

  HAL_TIM_Base_Init (Thumb, 74 bytes, Stack size 16 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM15_Init

  HAL_TIM_Base_MspInit (Thumb, 46 bytes, Stack size 8 bytes, stm32f0xx_hal_msp.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_Base_MspInit
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start_IT (Thumb, 82 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_Base_Start_IT))
  [Called By]

  - >> LIN_Init

  HAL_TIM_ConfigClockSource (Thumb, 220 bytes, Stack size 24 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> TIM_ITRx_SetConfig
  - >> TIM_ETR_SetConfig
  [Called By]
  - >> MX_TIM15_Init

  HAL_TIM_IC_CaptureCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_IRQHandler (Thumb, 362 bytes, Stack size 16 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_IRQHandler))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback ⇒ LIN_TimerProcess ⇒ LIN_WriteTxPortState ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIM_PeriodElapsedCallback
  - >> HAL_TIM_TriggerCallback
  - >> HAL_TIM_PWM_PulseFinishedCallback
  - >> HAL_TIM_OC_DelayElapsedCallback
  - >> HAL_TIM_IC_CaptureCallback
  - >> HAL_TIMEx_CommutCallback
  - >> HAL_TIMEx_BreakCallback
  [Called By]
  - >> TIM15_IRQHandler

  HAL_TIM_OC_DelayElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PWM_PulseFinishedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PeriodElapsedCallback (Thumb, 20 bytes, Stack size 8 bytes, lin.o(i.HAL_TIM_PeriodElapsedCallback))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_TIM_PeriodElapsedCallback ⇒ LIN_TimerProcess ⇒ LIN_WriteTxPortState ⇒ HAL_GPIO_Init
  [Calls]
  - >> LIN_TimerProcess
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_TriggerCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_TriggerCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_UARTEx_RxEventCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_RxISR_8BIT
  - >> UART_RxISR_16BIT

  HAL_UARTEx_WakeupCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_uart_ex.o(i.HAL_UARTEx_WakeupCallback))
  [Called By]

  - >> HAL_UART_IRQHandler

  HAL_UART_AbortReceive (Thumb, 128 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_AbortReceive))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_UART_AbortReceive ⇒ HAL_DMA_Abort
  [Calls]
  - >> HAL_DMA_GetError
  - >> HAL_DMA_Abort
  [Called By]
  - >> LIN_TimerProcess

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMAAbortOnError

  HAL_UART_IRQHandler (Thumb, 538 bytes, Stack size 24 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 116
  - Call Chain = HAL_UART_IRQHandler ⇒ UART_EndTransmit_IT ⇒ HAL_UART_TxCpltCallback ⇒ LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> HAL_DMA_Abort
  - >> HAL_UART_ErrorCallback
  - >> HAL_UARTEx_RxEventCallback
  - >> HAL_UARTEx_WakeupCallback
  - >> UART_EndTransmit_IT
  - >> UART_EndRxTransfer
  - >> HAL_DMA_Abort_IT
  [Called By]
  - >> USART2_IRQHandler
  - >> USART1_IRQHandler

  HAL_UART_Init (Thumb, 112 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  [Called By]
  - >> MX_USART2_UART_Init

  HAL_UART_MspInit (Thumb, 166 bytes, Stack size 48 bytes, stm32f0xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> HAL_UART_Init
  - >> HAL_LIN_Init

  HAL_UART_Receive (Thumb, 284 bytes, Stack size 56 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Receive))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_UART_Receive ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  - >> HAL_GetTick
  [Called By]
  - >> main

  HAL_UART_Receive_IT (Thumb, 96 bytes, Stack size 12 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Receive_IT))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> UART_Start_Receive_IT
  [Called By]
  - >> LIN_UartProcess
  - >> LIN_TimerProcess
  - >> LIN_Receive

  HAL_UART_RxCpltCallback (Thumb, 20 bytes, Stack size 8 bytes, lin.o(i.HAL_UART_RxCpltCallback))
  [Stack]

  - Max Depth = 84
  - Call Chain = HAL_UART_RxCpltCallback ⇒ LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> LIN_UartProcess
  [Called By]
  - >> UART_RxISR_8BIT
  - >> UART_RxISR_16BIT

  HAL_UART_Transmit (Thumb, 248 bytes, Stack size 48 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  - >> HAL_GetTick
  [Called By]
  - >> main

  HAL_UART_Transmit_IT (Thumb, 136 bytes, Stack size 12 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Transmit_IT))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_UART_Transmit_IT
  [Called By]
  - >> LIN_UartProcess
  - >> LIN_Transmit
  - >> LIN_TimerProcess

  HAL_UART_TxCpltCallback (Thumb, 20 bytes, Stack size 8 bytes, lin.o(i.HAL_UART_TxCpltCallback))
  [Stack]

  - Max Depth = 84
  - Call Chain = HAL_UART_TxCpltCallback ⇒ LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> LIN_UartProcess
  [Called By]
  - >> UART_EndTransmit_IT

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f051x8.o(RESET)

  LIN_CalcCheckSum (Thumb, 40 bytes, Stack size 8 bytes, lin.o(i.LIN_CalcCheckSum))
  [Stack]

  - Max Depth = 8
  - Call Chain = LIN_CalcCheckSum
  [Called By]
  - >> main
  - >> LIN_UartProcess

  LIN_GetDataLength (Thumb, 28 bytes, Stack size 0 bytes, lin.o(i.LIN_GetDataLength))
  [Called By]

  - >> LIN_SlaveIdRxCallback

  LIN_Init (Thumb, 76 bytes, Stack size 24 bytes, lin.o(i.LIN_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = LIN_Init ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_TIM_Base_Start_IT
  - >> __aeabi_uidivmod
  [Called By]
  - >> main

  LIN_ReadRxPortState (Thumb, 16 bytes, Stack size 8 bytes, lin.o(i.LIN_ReadRxPortState))
  [Stack]

  - Max Depth = 8
  - Call Chain = LIN_ReadRxPortState
  [Calls]
  - >> HAL_GPIO_ReadPin
  [Called By]
  - >> LIN_TimerProcess

  LIN_Receive (Thumb, 74 bytes, Stack size 24 bytes, lin.o(i.LIN_Receive))
  [Stack]

  - Max Depth = 44
  - Call Chain = LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> HAL_UART_Receive_IT
  [Called By]
  - >> LIN_SlaveIdRxCallback

  LIN_Reset (Thumb, 8 bytes, Stack size 0 bytes, lin.o(i.LIN_Reset))
  [Called By]

  - >> LIN_SlaveIdRxCallback

  LIN_RxCpltCallback (Thumb, 10 bytes, Stack size 0 bytes, main.o(i.LIN_RxCpltCallback))
  [Called By]

  - >> LIN_UartProcess

  LIN_SlaveIdRxCallback (Thumb, 66 bytes, Stack size 8 bytes, main.o(i.LIN_SlaveIdRxCallback))
  [Stack]

  - Max Depth = 52
  - Call Chain = LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> HAL_GPIO_TogglePin
  - >> LIN_Transmit
  - >> LIN_Reset
  - >> LIN_Receive
  - >> LIN_GetDataLength
  [Called By]
  - >> LIN_UartProcess

  LIN_TimerProcess (Thumb, 164 bytes, Stack size 16 bytes, lin.o(i.LIN_TimerProcess))
  [Stack]

  - Max Depth = 72
  - Call Chain = LIN_TimerProcess ⇒ LIN_WriteTxPortState ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Transmit_IT
  - >> HAL_UART_Receive_IT
  - >> HAL_UART_AbortReceive
  - >> __ARM_common_switch8
  - >> LIN_WriteTxPortState
  - >> LIN_ReadRxPortState
  [Called By]
  - >> HAL_TIM_PeriodElapsedCallback

  LIN_Transmit (Thumb, 74 bytes, Stack size 24 bytes, lin.o(i.LIN_Transmit))
  [Stack]

  - Max Depth = 36
  - Call Chain = LIN_Transmit ⇒ HAL_UART_Transmit_IT
  [Calls]
  - >> HAL_UART_Transmit_IT
  [Called By]
  - >> LIN_SlaveIdRxCallback

  LIN_UartProcess (Thumb, 178 bytes, Stack size 24 bytes, lin.o(i.LIN_UartProcess))
  [Stack]

  - Max Depth = 76
  - Call Chain = LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> LIN_SlaveIdRxCallback
  - >> LIN_RxCpltCallback
  - >> HAL_UART_Transmit_IT
  - >> HAL_UART_Receive_IT
  - >> __ARM_common_switch8
  - >> LIN_CalcCheckSum
  [Called By]
  - >> HAL_UART_TxCpltCallback
  - >> HAL_UART_RxCpltCallback

  LIN_WriteTxPortState (Thumb, 104 bytes, Stack size 32 bytes, lin.o(i.LIN_WriteTxPortState))
  [Stack]

  - Max Depth = 56
  - Call Chain = LIN_WriteTxPortState ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  - >> HAL_GPIO_DeInit
  - >> __aeabi_memclr4
  [Called By]
  - >> LIN_TimerProcess

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(i.NMI_Handler))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f051x8.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Handler
  [Calls]
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f051x8.o(RESET)

  SystemClock_Config (Thumb, 112 bytes, Stack size 104 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 232
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  SystemInit (Thumb, 2 bytes, Stack size 0 bytes, system_stm32f0xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f051x8.o(.text)

  TIM15_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.TIM15_IRQHandler))
  [Stack]

  - Max Depth = 104
  - Call Chain = TIM15_IRQHandler ⇒ HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback ⇒ LIN_TimerProcess ⇒ LIN_WriteTxPortState ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f051x8.o(RESET)

  TIM_Base_SetConfig (Thumb, 126 bytes, Stack size 16 bytes, stm32f0xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  TIM_ETR_SetConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f0xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  UART_AdvFeatureConfig (Thumb, 204 bytes, Stack size 4 bytes, stm32f0xx_hal_uart.o(i.UART_AdvFeatureConfig))
  [Stack]

  - Max Depth = 4
  - Call Chain = UART_AdvFeatureConfig
  [Called By]
  - >> HAL_UART_Init
  - >> HAL_LIN_Init

  UART_CheckIdleState (Thumb, 98 bytes, Stack size 24 bytes, stm32f0xx_hal_uart.o(i.UART_CheckIdleState))
  [Stack]

  - Max Depth = 64
  - Call Chain = UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Init
  - >> HAL_LIN_Init

  UART_SetConfig (Thumb, 312 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 120
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetPCLK1Freq
  - >> __aeabi_uidivmod
  [Called By]
  - >> HAL_UART_Init
  - >> HAL_LIN_Init

  UART_Start_Receive_IT (Thumb, 128 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.UART_Start_Receive_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_Start_Receive_IT
  [Called By]
  - >> HAL_UART_Receive_IT

  UART_WaitOnFlagUntilTimeout (Thumb, 192 bytes, Stack size 40 bytes, stm32f0xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 40
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  - >> UART_CheckIdleState

  USART1_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 124
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ UART_EndTransmit_IT ⇒ HAL_UART_TxCpltCallback ⇒ LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f051x8.o(RESET)

  USART2_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 124
  - Call Chain = USART2_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ UART_EndTransmit_IT ⇒ HAL_UART_TxCpltCallback ⇒ LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f051x8.o(RESET)

  __ARM_common_ll_muluu (Thumb, 50 bytes, Stack size 16 bytes, stm32f0xx_hal_rcc.o(i.__ARM_common_ll_muluu))
  [Stack]

  - Max Depth = 16
  - Call Chain = __ARM_common_ll_muluu
  [Called By]
  - >> HAL_RCC_GetSysClockFreq

  __ARM_common_switch8 (Thumb, 26 bytes, Stack size 8 bytes, lin.o(i.__ARM_common_switch8))
  [Stack]

  - Max Depth = 8
  - Call Chain = __ARM_common_switch8
  [Called By]
  - >> LIN_UartProcess
  - >> LIN_TimerProcess

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 266 bytes, Stack size 16 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 248
  - Call Chain = main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  - >> HAL_LIN_SendBreak
  - >> HAL_Init
  - >> HAL_Delay
  - >> SystemClock_Config
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init
  - >> MX_TIM15_Init
  - >> MX_GPIO_Init
  - >> LIN_Init
  - >> LIN_CalcCheckSum
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  MX_GPIO_Init (Thumb, 98 bytes, Stack size 40 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_TIM15_Init (Thumb, 98 bytes, Stack size 32 bytes, main.o(i.MX_TIM15_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = MX_TIM15_Init ⇒ HAL_TIM_ConfigClockSource ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 50 bytes, Stack size 8 bytes, main.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 144
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_LIN_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> HAL_LIN_Init
  [Called By]
  - >> main

  MX_USART2_UART_Init (Thumb, 48 bytes, Stack size 8 bytes, main.o(i.MX_USART2_UART_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = MX_USART2_UART_Init ⇒ HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uldivmod ⇒ __aeabi_llsl
  [Calls]
  - >> HAL_UART_Init
  [Called By]
  - >> main

  TIM_ITRx_SetConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_TI1_ConfigInputStage (Thumb, 36 bytes, Stack size 8 bytes, stm32f0xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_TI2_ConfigInputStage (Thumb, 40 bytes, Stack size 8 bytes, stm32f0xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  UART_DMAAbortOnError (Thumb, 20 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMAAbortOnError
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f0xx_hal_uart.o(i.HAL_UART_IRQHandler)

  UART_EndRxTransfer (Thumb, 50 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.UART_EndRxTransfer))
  [Called By]

  - >> HAL_UART_IRQHandler

  UART_EndTransmit_IT (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.UART_EndTransmit_IT))
  [Stack]

  - Max Depth = 92
  - Call Chain = UART_EndTransmit_IT ⇒ HAL_UART_TxCpltCallback ⇒ LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> HAL_UART_TxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_RxISR_16BIT (Thumb, 120 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.UART_RxISR_16BIT))
  [Stack]

  - Max Depth = 100
  - Call Chain = UART_RxISR_16BIT ⇒ HAL_UART_RxCpltCallback ⇒ LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  - >> HAL_UARTEx_RxEventCallback
  [Address Reference Count : 1]
  - stm32f0xx_hal_uart.o(i.UART_Start_Receive_IT)

  UART_RxISR_8BIT (Thumb, 120 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.UART_RxISR_8BIT))
  [Stack]

  - Max Depth = 100
  - Call Chain = UART_RxISR_8BIT ⇒ HAL_UART_RxCpltCallback ⇒ LIN_UartProcess ⇒ LIN_SlaveIdRxCallback ⇒ LIN_Receive ⇒ HAL_UART_Receive_IT ⇒ UART_Start_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  - >> HAL_UARTEx_RxEventCallback
  [Address Reference Count : 1]
  - stm32f0xx_hal_uart.o(i.UART_Start_Receive_IT)

  UART_TxISR_16BIT (Thumb, 64 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.UART_TxISR_16BIT))
  [Address Reference Count : 1]

  - stm32f0xx_hal_uart.o(i.HAL_UART_Transmit_IT)

  UART_TxISR_8BIT (Thumb, 60 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.UART_TxISR_8BIT))
  [Address Reference Count : 1]

  - stm32f0xx_hal_uart.o(i.HAL_UART_Transmit_IT)

  ### Undefined Global Symbols